Using the F200 and NanoQuant plate for 260/280 determinations
1. Combine samples and assay components in a microplate as per protocol.
2. Turn on the Tecan F200 and open the i-Control software.
3. In the menu select NanoQuant as the plate to be read.   

4. Select “Individual blanking” and load each well with a drop of water (or buffer) to read.

5. Customize the data output depending on whether you’re doing DNA, RNA, or protein readings.  Select the appropriate sample type, load the wells and read again. The data will dump automatically into an Excel spreadsheet.